; ************************************************************
; ************************************************************
; **  Filename: Chipset_System.inf                          **
; **  Abstract: Assigns the null driver to System           **
; **            devices for yellow-bang removal.            **
; ************************************************************
; ************************************************************


[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGUID={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
CatalogFile=Chipset.cat
DriverVer=02/25/2014, 10.0.13

[SourceDisksNames]

[SourceDisksFiles]

[ControlFlags]
ExcludeFromSelect=*

[PackageInfo]
Name=Chipset

[Manufacturer]
%INTEL%=INTEL,NT,NTamd64

[INTEL.NT]
;IvyTown
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E1E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E1F
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E20
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E21
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E22
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E23
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E24
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E25
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E26
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E27
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E28
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E29
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E2A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E2C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E30
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E71
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E80
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E90
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EA0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EA8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EAA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EAB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EAC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EAD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0ECA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_1D68
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0ED8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0ED9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EDC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EDD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EDE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EDF
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EFA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EFB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EFC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EFD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E38
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E60
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E10
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E13
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E17
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E18
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E1C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E6A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E6B
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E6C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E6D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E79
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E68
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E32
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E33
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E3A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E40
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E87
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E36
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E37
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E81
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E1D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E34
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E7D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EEA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EEB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EEC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EED
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EEE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E45
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E47
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E85
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E95
;Haswell-E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F10
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F11
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F12
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F13
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F14
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F15
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F16
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F17
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F18
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F19
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1B
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1F
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F20
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F21
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F22
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F23
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F24
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F25
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F26
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F27
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F28
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F29
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F2A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F2C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F30
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F32
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F33
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F34
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F36
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F37
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F38
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F39
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F3A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F3E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F3F
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F40
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F41
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F43
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F45
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F46
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F47
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F60
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F68
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6B
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6F
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F70
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F71
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F76
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F78
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F79
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F7D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F7E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F80
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F81
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F83
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F85
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F86
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F87
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F88
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F8A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F90
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F93
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F95
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F96
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F98
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F99
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F9A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F9C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FA0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FA8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAF
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBF
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FC0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FED
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEF
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFE
;Wellsburg
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_8D7C


[INTEL.NTamd64]
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E1E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E1F
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E20
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E21
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E22
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E23
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E24
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E25
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E26
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E27
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E28
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E29
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E2A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E2C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E30
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E71
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E80
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E90
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EA0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EA8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EAA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EAB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EAC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EAD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EB7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EC9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0ECA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EE9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_1D68
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0ED8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0ED9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EDC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EDD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EDE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EDF
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EFA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EFB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EFC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EFD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E38
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E60
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E10
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E13
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E17
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E18
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E1C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EF5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E6A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E6B
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E6C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E6D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E79
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E68
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E32
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E33
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E3A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E40
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E87
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E36
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E37
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E81
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E1D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E34
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E7D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EEA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EEB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EEC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EED
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0EEE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E45
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E47
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E85
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_0E95
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F10
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F11
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F12
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F13
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F14
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F15
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F16
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F17
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F18
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F19
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1B
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F1F
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F20
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F21
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F22
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F23
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F24
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F25
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F26
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F27
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F28
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F29
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F2A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F2C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F30
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F32
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F33
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F34
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F36
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F37
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F38
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F39
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F3A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F3E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F3F
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F40
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F41
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F43
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F45
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F46
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F47
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F60
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F68
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6B
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F6F
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F70
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F71
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F76
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F78
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F79
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F7D
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F7E
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F80
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F81
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F83
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F85
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F86
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F87
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F88
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F8A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F90
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F93
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F95
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F96
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F98
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F99
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F9A
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2F9C
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FA0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FA8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FAF
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FB9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FBF
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FC0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FD7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FE9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FED
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FEF
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF0
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF1
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF2
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF3
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF4
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF5
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF6
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF7
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF8
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FF9
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFA
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFB
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFC
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFD
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_2FFE
%IntelDeviceDesc%=Needs_NO_DRV, , PCI\VEN_8086&DEV_8D7C


[Needs_NO_DRV]
Include=machine.inf
Needs=NO_DRV

[Needs_NO_DRV.Services]
Include=machine.inf
Needs=NO_DRV.Services

[Strings]
INTEL="Intel"
IntelDeviceDesc="Intel Device"


; Copyright (c) 2003-2014 Intel Corporation
; 
; ********************************************************************************
; Intel is making no claims of usability, efficacy or warranty.
; ********************************************************************************
; Information in this document is provided in connection with Intel products. No
; license, express or implied, by estoppel or otherwise, to any intellectual
; property rights is granted by this document. Intel assumes no liability
; whatsoever, and Intel disclaims any express or implied warranty, relating to
; sale and/or use of Intel products including liability or warranties relating to
; fitness for a particular purpose, merchantability, or infringement of any
; patent, copyright or other intellectual property right. Intel products are not
; intended for use in medical, life saving, or life sustaining applications.
; ********************************************************************************
; Intel Corporation disclaims all warranties and liabilities for the use of this
; document and the information contained herein, and assumes no responsibility for
; any errors which may appear in this document, nor does Intel make a commitment
; to update the information contained herein. Intel reserves the right to make
; changes to this document at any time, without notice.
; ********************************************************************************
; ********************************************************************************
; 
; * Third-party brands and names are the property of their respective owners.
